
Wave flume test on 3/20/2023


**Flume dimensions**

L = 432cm, W = 30 cm, H = 45cm

**PVC pipe array – high density**

****

**PVC pipe array – low density**



**Wave gauge location**

For the first wave gauge at x = 0cm, the second wave gauge is at x = 165cm and the third wave gauge is at x = 264cm. Note that in the videos, the wave gauges are located at 170”, 105”, and 66”, respectively. These numbers are the readings on the ruler but not the x coordinates.

**Case conditions**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| case | Pipe array | Xp (cm) | Depth (cm) | Amplitude | Frequency |
| 1\_BL | Off | NA | 9.2 | Large | Low |
| 1\_LD | Low density | 172.7 | 9.4 | Large | Low |
| 1\_HD | High density | 172.7 | 9.8 | Large | Low |
| 2\_BL | Off | NA | 9.0 | Small | High |
| 2\_LD | Low density | 172.7 | 8.8 | Small | High |
| 2\_HD | High density | 172.7 | 8.6 | Small | High |

Note:

The amplitude of the wavemaker was not measured. The wave frequency can be obtained by frequency-domain analysis.